//
// Copyright (C) 1999, 2000, 2001, 2002, 2003, 2004, 2005 Yokogawa Electric Corporation.
// All rights reserved.
// 
// Redistribution and use of this software in source and binary
// forms, with or without modification, are permitted provided that
// the following conditions and disclaimer are agreed and accepted
// by the user:
// 
// 1. Redistributions of source code must retain the above copyright
//    notice, this list of conditions and the following disclaimer.
// 
// 2. Redistributions in binary form must reproduce the above copyright
//    notice, this list of conditions and the following disclaimer in
//    the documentation and/or other materials provided with
//    the distribution.
// 
// 3. Neither the names of the copyrighters, the name of the project
//    which is related to this software (hereinafter referred to as
//    "project") nor the names of the contributors may be used to
//    endorse or promote products derived from this software without
//    specific prior written permission.
// 
// 4. No merchantable use may be permitted without prior written
//    notification to the copyrighters.
// 
// 5. The copyrighters, the project and the contributors may prohibit
//    the use of this software at any time.
// 
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHTERS, THE PROJECT AND
// CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING
// BUT NOT LIMITED THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
// FOR A PARTICULAR PURPOSE, ARE DISCLAIMED.  IN NO EVENT SHALL THE
// COPYRIGHTERS, THE PROJECT OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT,
// INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
// (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
// SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
// HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT,
// STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING
// IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
// POSSIBILITY OF SUCH DAMAGE.
//
// Copyright (C) 1999, 2000, 2001, 2002, 2003, 2004, 2005 Yokogawa Electric Corporation.
// All rights reserved.
// 
// Redistribution and use of this software in source and binary
// forms, with or without modification, are permitted provided that
// the following conditions and disclaimer are agreed and accepted
// by the user:
// 
// 1. Redistributions of source code must retain the above copyright
//    notice, this list of conditions and the following disclaimer.
// 
// 2. Redistributions in binary form must reproduce the above copyright
//    notice, this list of conditions and the following disclaimer in
//    the documentation and/or other materials provided with
//    the distribution.
// 
// 3. Neither the names of the copyrighters, the name of the project
//    which is related to this software (hereinafter referred to as
//    "project") nor the names of the contributors may be used to
//    endorse or promote products derived from this software without
//    specific prior written permission.
// 
// 4. No merchantable use may be permitted without prior written
//    notification to the copyrighters.
// 
// 5. The copyrighters, the project and the contributors may prohibit
//    the use of this software at any time.
// 
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHTERS, THE PROJECT AND
// CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING
// BUT NOT LIMITED THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
// FOR A PARTICULAR PURPOSE, ARE DISCLAIMED.  IN NO EVENT SHALL THE
// COPYRIGHTERS, THE PROJECT OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT,
// INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
// (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
// SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
// HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT,
// STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING
// IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
// POSSIBILITY OF SUCH DAMAGE.
//
// $TAHI: ct/nd/adrsolvQueuMulti.def,v 1.7 2004/04/02 02:28:22 akisada Exp $

#include "nd.def"

//----------------------------------------------------------------------
// echo-request
//	TN(link-local) ==> NUT(link-local)
//
//----------------------------------------------------------------------
FEM_icmp6_echo_request(echo_request_from_tn, _HETHER_tn2nut,
	{
	 _SRC(tnv6());
	 _DST(nutv6());},
	{
	 Identifier=0x6000;
	 SequenceNumber=10;
	 payload=echo_data_tn;
	}
)

//----------------------------------------------------------------------
// echo-reply
//	NUT(link-local) ==> TN(link-local)
//
//----------------------------------------------------------------------
FEM_icmp6_echo_reply(echo_reply_to_tn, _HETHER_nut2tn,
	{
	 _SRC(nutv6());
	 _DST(tnv6());
	},
	{
	 Identifier=0x6000;
	 SequenceNumber=10;
	 payload=echo_data_tn;
	}
)

//----------------------------------------------------------------------
Payload echo_data_tn {
	data=repeat(0x11,10);
}

//----------------------------------------------------------------------
// multicast NS
//	NUT(link-local) ==> tn(solicited-node[link-local])
//	target=TN(link-local)
//	w/ SLLA
//
//----------------------------------------------------------------------
FEM_icmp6_ns(multicast_ns_to_tn, _HETHER_nut2tnsolnode,
        {
         _SRC(oneof(NUT_GLOBAL, nutv6()));
         _DST(_IPV6_SOLNODE_MCAST(tnv6()));
         HopLimit=255;
        },
        {
         TargetAddress=tnv6();
         option=_SLLOPT_nut;
        }
)

//----------------------------------------------------------------------
// unicast NA
//	TN(link-local) ==> NUT(link-local)
//	r=0, s=1, o=0
//	target=TN(link-local)
//	w/ TLLA
//
//----------------------------------------------------------------------
FEM_icmp6_na(na_from_tn, _HETHER_tn2nut,
        {
         _SRC(tnv6());
         _DST(nutv6());
         HopLimit=255;
        },
        {
         RFlag=0;
         SFlag=1;
         OFlag=1;
         TargetAddress=tnv6();
         option=_TLLOPT_tn;
        }
)

//----------------------------------------------------------------------
_HETHER_define(hether_x2nut, ether(A0N_MAC_ADDR), nutether())
_HETHER_define(hether_nut2x, nutether(), ether(A0N_MAC_ADDR))
_HETHER_define(hether_nut2xsolnode, nutether(),
	_ETHER_SOLNODE_MCAST(v6ether(A0N_MAC_ADDR)))
_TLLOPT_define(tllopt_x, ether(A0N_MAC_ADDR))

//----------------------------------------------------------------------
// echo-request
//	X(link-local) ==> NUT(link-local)
//
//----------------------------------------------------------------------
FEM_icmp6_echo_request(echo_request_from_x, hether_x2nut,
	{
	 _SRC(v6ether(A0N_MAC_ADDR));
	 _DST(nutv6());},
	{
	 Identifier=0x7000;
	 SequenceNumber=20;
	 payload=echo_data_x;
	}
)

//----------------------------------------------------------------------
// echo-reply
//	NUT(link-local) ==> X(link-local)
//
//----------------------------------------------------------------------
FEM_icmp6_echo_reply(echo_reply_to_x, hether_nut2x,
	{
	 _SRC(nutv6());
	 _DST(v6ether(A0N_MAC_ADDR));
	},
	{
	 Identifier=0x7000;
	 SequenceNumber=20;
	 payload=echo_data_x;
	}
)

//----------------------------------------------------------------------
Payload echo_data_x {
	data=repeat(0x22,10);
}

//----------------------------------------------------------------------
// multicast NS
//	NUT(link-local) ==> X(solicited-node[link-local])
//	target=X(link-local)
//	w/ SLLA
//
//----------------------------------------------------------------------
FEM_icmp6_ns(multicast_ns_to_x, hether_nut2xsolnode,
        {
         _SRC(oneof(NUT_GLOBAL, nutv6()));
         _DST(_IPV6_SOLNODE_MCAST(v6ether(A0N_MAC_ADDR)));
         HopLimit=255;
        },
        {
         TargetAddress=v6ether(A0N_MAC_ADDR);
         option=_SLLOPT_nut;
        }
)

//----------------------------------------------------------------------
// unicast NA
//	X(link-local) ==> NUT(link-local)
//	r=0, s=1, o=1
//	target=X(link-local)
//	w/ TLLA
//
//----------------------------------------------------------------------
FEM_icmp6_na(na_from_x, hether_x2nut,
        {
         _SRC(v6ether(A0N_MAC_ADDR));
         _DST(nutv6());
         HopLimit=255;
        },
        {
         RFlag=0;
         SFlag=1;
         OFlag=1;
         TargetAddress=v6ether(A0N_MAC_ADDR);
         option=tllopt_x;
        }
)

//----------------------------------------------------------------------
